#PACE: Start of Constraints generated by PACE

#PACE: Start of PACE I/O Pin Assignments

NET "bus_a<4>"  LOC = "P28"  ; # A12
NET "bus_a<3>"  LOC = "P27"  ;  # A11
NET "bus_a<2>"  LOC = "P26"  ;  # A10
NET "bus_a<1>"  LOC = "P25"  ; # A9
NET "bus_a<0>"  LOC = "P24"  ; # A8

NET "bus_d<7>"  LOC = "P4"  ;
NET "bus_d<6>"  LOC = "P3"  ;
NET "bus_d<5>"  LOC = "P2"  ;
NET "bus_d<4>"  LOC = "P1"  ;
NET "bus_d<3>"  LOC = "P44"  ;
NET "bus_d<2>"  LOC = "P43"  ;
NET "bus_d<1>"  LOC = "P42"  ;
NET "bus_d<0>"  LOC = "P40"  ;

NET "reset_n"  LOC = "P8"  ;

NET "rom_bank<7>"  LOC = "P18"  ; # XA19
NET "rom_bank<6>"  LOC = "P19"  ; # XA18
NET "rom_bank<5>"  LOC = "P20"  ; # XA17
NET "rom_bank<4>"  LOC = "P38"  ; # XA16
NET "rom_bank<3>"  LOC = "P37"  ; # XA15
NET "rom_bank<2>"  LOC = "P36"  ; # XA14
NET "rom_bank<1>"  LOC = "P33"  ; # XA13
NET "rom_bank<0>"  LOC = "P29"  ; # XA12

NET "rom_cs_n"  LOC = "P35"  ;
NET "rom_oe_n"  LOC = "P34"  ;


#PACE: Start of PACE Area Constraints

#PACE: Start of PACE Prohibit Constraints

#PACE: End of Constraints generated by PACE
