ColecoVision ROM Cartridge
--------------------------
This board is made to be used with one ColecoVision ROM file (up to 16Ko).
For the moment, only one file can be stored to the EProm (no bank switching or bank selection).

This PCB corresponds to the remake of my previous version (24/10/2008).


Files
-----
Coleco-Rom-Cart.sch : Schematics (Eagle 5.0.0)
Coleco-Rom-Cart.brd : PCB (Eagle 5.0.0)

ColecoVision-Rom-Cart-component-layer.png : 300dpi Component layer (top side) 
ColecoVision-Rom-Cart-copper-layer.png : 300dpi Component layer (bottom side) 
ColecoVision-Rom-Cart-PCB.png : 300dpi full board
ColecoVision-Rom-Cart.png : 300dpi schematics

Part list
---------
IC1 : 27C256
IC2 : 74LS21

Usage
-----
Just 'flash' one 2Ko, 4Ko, 8K or 16Ko files to the UVProm and plug-in the cartridge into the console.


Any suggestions or comments are welcomed (contact buzz.computer.free.fr)

Enjoy !

Buzz